**# Title:**

Fix incorrect reference to "Memory Aggregator Device"

**# Status:**

Draft

**# Document:**

ACPI 6.4 specification

**# License:**

SPDX-License-Identifier: CC-BY-4.0

**# Submitters:**

* Samer El-Haj-Mahmoud, ARM
* Christopher Jones, ARM
* TianoCore Community (<https://www.tianocore.org>)

**# Summary of the change**

Fix incorrect field name in Table 5.80

**# Benefits of the change**

ACPI 6.4 specification, Table 5.80 the name of the last field at offset 40 is "Memory Aggregator Device Structure [n]". This is incorrect, as the structure referenced in table 5.81 is "Common Memory Device", not "Memory Aggregator Device"

**# Impact of the change**

* Just a spec reference / clarification to match the SDEI spec. No impact to OS or FW implementations

**# Detailed description of the change [normative updates]**

* Insertions in **green**
* Removals in ~~red~~

Table 5.80: Platform Memory Topology Table

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Byte Length** | **Byte Offset** | **Description** |
| .. | … | … | … |
| Memory ~~Aggregator~~ Device  Structure [n] | \_\_ | 40 | list of memory device structures for the platform. See  Table 5.81 below. |